{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["mt6765"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"mt6765","index":0,"n_rows":16,"n_cols":60,"rows_kept":16,"merged":[[0,0,2,0],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,2,4],[0,5,2,5],[0,6,2,6],[0,7,2,7],[0,8,2,8],[0,9,1,59]],"flags":["formulas_cached_only"]}
["Vendor","Part Number","Type","Mode","Density (Mb)","Board ID","NAND/eMMC ID","FW ID","Nand Page Size (B)","MT6765"]
[]
[{"$nulls":9},"CONA_VAL","CHN0_CONA_VAL","CHN1_CONA_VAL","CONF_VAL","CONH_VAL","FREQUENCY","TRAS","TRP","TRPAB","TRC","TRFC","TRFCPB","TXP","TRTP","TRCD","TWR","TWTR","TRRD","TFAW","TRTW_ODT_OFF","TRTW_ODT_ON","REFCNT","REFCNT_FR_CLK","TXREFCNT","TZQCS","TRTPD","TWTPD","TMRR2W_ODT_OFF","TMRR2W_ODT_ON","CHIP_ID","TRAS_05T","TRP_05T","TRPAB_05T","TRC_05T","TRFC_05T ","TRFCPB_05T","TXP_05T","TRTP_05T","TRCD_05T","TWR_05T","TWTR_05T","TRRD_05T","TFAW_05T","TRTW_ODT_OFF_05T","TRTW_ODT_ON_05T","TRTPD_05T ","TWTPD_05T ","TMRR2W_ODT_OFF_05T ","TMRR2W_ODT_ON_05T ","MODE_REG5","PIN_MUX_TYPE"]
["Hynix ","H9TQ26ADFTBCUR","MCP(eMMC+LPDDR3)","R0_BYTE+R1_NORMAL","16384+8192","MT6765_EVB","0x90014A484247346132",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",0]
["Hynix ","H9TQ27ADFTMCUR","MCP(eMMC+LPDDR3)","R0_BYTE+R1_NORMAL","16384+8192","MT6765_EVB","0x90014A68423861503E",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",0]
["Hynix ","H9TQ17ABJTCCUR","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","8192+8192","MT6765_EVB","0x90014A484147346132",null,null,"0xa053a056","0x0044a053","0x0044a053","0x00421000","0x44440003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",0]
["Samsung","KMQE60013M_B318","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","8192+8192","MT6765_EVB","0x150100514536334D42",null,null,"0xa053a056","0x0044a053","0x0044a053","0x00421000","0x44440003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000001",0]
["Samsung","KMGD6001BM_B421","MCP(eMMC+LPDDR3)","R0_BYTE+R1_NORMAL","16384+8192","MT6765_EVB","0x150100474436424D42",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000001",0]
["Micron","MT29TZZZ5D7DKFRL_107","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","8192+8192","MT6765_EVB","0x13014E53304A394137",null,null,"0xa053a056","0x0044a053","0x0044a053","0x00421000","0x44440003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x000000FF",0]
["Micron","MT29TZZZ7D7DKLAH_107","MCP(eMMC+LPDDR3)","R0_BYTE+R1_NORMAL","16384+8192","MT6765_EVB","0x13014E53304A394237",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x000000FF",0]
["Hynix ","H9HP52ACPMMDAR","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL","16384+16384","MT6765_EVB","0x90014A484347386134",null,null,"0xF053F154","0x0444F051","0x0444F051","0x00421000","0x44440003",{"$nulls":24},"mt6765",{"$nulls":19},"0x00000006",0]
["Hynix ","H9CCNNNBJTALAR_NUD","Discrete LPDDR3","R0_NORMAL+R1_NORMAL","8192+8192","MT6765_EVB",{"$nulls":3},"0xa053a056","0x0044a053","0x0044a053","0x00421000","0x44440003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",1]
["Samsung","KMRD60014M_B512","MCP(eMMC+LPDDR3)","R0_BYTE+R1_BYTE","16384+16384","MT6765_EVB","0x150100524436344D42",null,null,"0xa0a3a0a6","0x0088a0a3","0x0088a0a3","0x04210000","0x88880003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000001",0]
["Biwin","BWMD8X32H2A_LP4","Discrete LPDDR4","R0_NORMAL+R1_NORMAL","12288+12288","MT6765_EVB",{"$nulls":3},"0xF053F154","0x0433F051","0x0433F051","0x00421000","0x33330003",{"$nulls":24},"mt6765",{"$nulls":19},"0x000000FF",0]
["Hynix ","H9TQ27ADFTMCUR_KUM","MCP(eMMC+LPDDR3)","R0_BYTE+R1_NORMAL","16384+8192","MT8768_EVB","0x90014A68423861503E",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",0]
["Hynix ","H9TQ17ABJTCCUR_KUM","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","8192+8192","MT8768_EVB","0x90014A484147346132",null,null,"0xa053a056","0x0044a053","0x0044a053","0x00421000","0x44440003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6765",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000006",0]