{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["mt6771"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"mt6771","index":0,"n_rows":16,"n_cols":60,"rows_kept":16,"merged":[[0,0,2,0],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,2,4],[0,5,2,5],[0,6,2,6],[0,7,2,7],[0,8,2,8],[0,9,1,59]],"flags":["formulas_cached_only"]}
["Vendor","Part Number","Type","Mode","Density (Mb)","Board ID","NAND/eMMC ID","FW ID","Nand Page Size (B)","MT6771"]
[]
[{"$nulls":9},"CONA_VAL","CHN0_CONA_VAL","CHN1_CONA_VAL","CONF_VAL","CONH_VAL","FREQUENCY","TRAS","TRP","TRPAB","TRC","TRFC","TRFCPB","TXP","TRTP","TRCD","TWR","TWTR","TRRD","TFAW","TRTW_ODT_OFF","TRTW_ODT_ON","REFCNT","REFCNT_FR_CLK","TXREFCNT","TZQCS","TRTPD","TWTPD","TMRR2W_ODT_OFF","TMRR2W_ODT_ON","CHIP_ID","TRAS_05T","TRP_05T","TRPAB_05T","TRC_05T","TRFC_05T ","TRFCPB_05T","TXP_05T","TRTP_05T","TRCD_05T","TWR_05T","TWTR_05T","TRRD_05T","TFAW_05T","TRTW_ODT_OFF_05T","TRTW_ODT_ON_05T","TRTPD_05T ","TWTPD_05T ","TMRR2W_ODT_OFF_05T ","TMRR2W_ODT_ON_05T ","MODE_REG5","PIN_MUX_TYPE"]
["Hynix ","H9HP52ACPMMDAR","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL","16384+16384","MT6771_EVB","0x90014A484347386134",null,null,"0xF053F154","0x0444F051","0x0444F051","0x00421000","0x44440003",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000006",0]
["Samsung","KMDH6001DM_B422","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL","16384+16384","MT6771_EVB","0x150100444836444D42",null,null,"0xF053F154","0x0444F051","0x0444F051","0x00421000","0x44440003",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000001",0]
["Hynix ","H9TQ26ADFTBCUR","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","16384+8192","MT6771_EVB","0x90014A484247346132",null,null,"0xa063a066","0x0048a063","0x0048a063","0x04210000","0x48480003",933,11,6,1,20,86,30,0,2,7,12,7,3,14,6,6,112,101,101,41,10,11,8,10,"mt6771",0,1,1,1,0,0,1,1,1,1,0,0,1,1,1,0,0,0,0,"0x00000006",0]
["Samsung","KMRX60014M_B614","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","16384+16384","MT6771_EVB","0x150100525836344D42",null,null,"0xa0a3a0a6","0x0088a0a3","0x0088a0a3","0x04210000","0x88880003",933,11,6,1,20,86,30,0,2,7,12,7,3,14,6,6,112,101,101,41,10,11,0,0,"mt6771",0,1,1,1,0,0,1,1,1,1,0,0,1,1,1,0,0,0,0,"0x00000001",0]
["Hynix ","H28U74301AMR","Discrete LPDR4X","R0_NORMAL+R1_NORMAL","16384+16384","MT6771_EVB",{"$nulls":3},"0xF053F154","0x0444F051","0x0444F051","0x00000000","0x44440003",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000006",0]
["Micron","MT53B512M32D2NP","Discrete LPDDR4","R0_NORMAL+R1_NORMAL","8192+8192","MT8183_EVB",{"$nulls":3},"0xA053A154","0x0400A051","0x0400A051","0x00000000","0x00000003",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000006",0]
["Samsung","KMRD60014M_B512","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","16384+16384","MT6771_EVB","0x150100524436344D42",null,null,"0xa0a3a0a6","0x0088a0a3","0x0088a0a3","0x04210000","0x88880003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6771",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000001",0]
["Samsung","KM3H6001CM_B515","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6771_EVB","0x150100334836434D42",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000001",0]
["Samsung","KM3V6001CM_B705","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6771_EVB","0x150100335636434D42",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000001",0]
["Samsung","KMGD6001BM_B421","MCP(eMMC+LPDDR3)","R0_NORMAL+R1_NORMAL","16384+8192","MT6771_EVB","0x150100474436424D42",null,null,"0xA063A066","0x0048A063","0x0048A063","0x04210000","0x48480003",933,null,6,1,20,{"$nulls":4},7,{"$nulls":14},"mt6771",null,1,1,1,{"$nulls":4},1,{"$nulls":10},"0x00000001",0]
["Samsung","KM2V7001CM_B706","MCP(UFS+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6771_EVB","0x4b4d325637303031434d2d42373036",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",{"$nulls":24},"mt6771",{"$nulls":19},"0x00000001",0]
["Foresee","NCEPQCAM5_3216","MCP(eMMC+LPDDR4)","R0_NORMAL+R1_NORMAL","8192+8192","MT6771_EVB","0x880103534C44333262",null,null,"0xA053A154","0x0422A051","0x0422A051","0x00421000","0x22220003",{"$nulls":24},"mt6771",{"$nulls":19},"0x000000FF",0]
["Micron","MT29VZZZ7D8DQFSL_046W_9J8","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL",24576,"MT6771_EVB","0x13014E53304A394A38",null,null,"0x1100114","0x04660014","0x04660014","0x00421000","0x66660013",{"$nulls":5},"mt6771",{"$nulls":4},"0x000000FF",0,{"$nulls":12},"mt6771",{"$nulls":19},"0x000000FF",0]