{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["mt6779"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"mt6779","index":0,"n_rows":8,"n_cols":60,"rows_kept":8,"merged":[[0,0,2,0],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,2,4],[0,5,2,5],[0,6,2,6],[0,7,2,7],[0,8,2,8],[0,9,1,59]],"flags":["formulas_cached_only"]}
["Vendor","Part Number","Type","Mode","Density (Mb)","Board ID","NAND/eMMC ID","FW ID","Nand Page Size (B)","MT6779"]
[]
[{"$nulls":9},"CONA_VAL","CHN0_CONA_VAL","CHN1_CONA_VAL","CONF_VAL","CONH_VAL","FREQUENCY","TRAS","TRP","TRPAB","TRC","TRFC","TRFCPB","TXP","TRTP","TRCD","TWR","TWTR","TRRD","TFAW","TRTW_ODT_OFF","TRTW_ODT_ON","REFCNT","REFCNT_FR_CLK","TXREFCNT","TZQCS","TRTPD","TWTPD","TMRR2W_ODT_OFF","TMRR2W_ODT_ON","CHIP_ID","TRAS_05T","TRP_05T","TRPAB_05T","TRC_05T","TRFC_05T ","TRFCPB_05T","TXP_05T","TRTP_05T","TRCD_05T","TWR_05T","TWTR_05T","TRRD_05T","TFAW_05T","TRTW_ODT_OFF_05T","TRTW_ODT_ON_05T","TRTPD_05T ","TWTPD_05T ","TMRR2W_ODT_OFF_05T ","TMRR2W_ODT_ON_05T ","MODE_REG5","PIN_MUX_TYPE"]
["Samsung","KM2V7001CM_B706","MCP(UFS+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6779_EVB","0x4b4d325637303031434d2d42373036",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",{"$nulls":24},"mt6779",{"$nulls":19},"0x00000001",0]
["Samsung","KM2V7001CM_B706_EMMC","Discrete LPDR4X","R0_NORMAL+R1_BYTE","16384+32768","MT6779_EVB",{"$nulls":3},"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",{"$nulls":24},"mt6779",{"$nulls":19},"0x00000001",0]
["Samsung","KM8V7001JA_B813","MCP(UFS+LPDR4X)","R0_BYTE+R1_BYTE","32768+32768","MT6779_EVB","0x4b4d3856373030314a412d42383133",null,null,"0x03530154","0x0488005D","0x0488005D","0x00421000","0x88880033",{"$nulls":5},"mt6779",{"$nulls":4},"0x00000001",0,{"$nulls":12},"mt6779",{"$nulls":19},"0x00000001",0]
["Hynix ","H9HP52ACPMADAR","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL","16384+16384","MT6779_EVB","0x90014A68433861503E",null,null,"0xF053F154","0x0444F051","0x0444F051","0x04210000","0x44440003",{"$nulls":5},"mt6779",{"$nulls":4},"0x00000006",0,{"$nulls":12},"mt6779",{"$nulls":19},"0x00000006",0]
["Micron","MT29VZZZAD9DQKSM_046_W_9K9","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_NORMAL","16384+16384","MT6779_EVB","0x13014E53304A394B39",null,null,"0xF053F154","0x0444F051","0x0444F051","0x04210000","0x44440003",{"$nulls":5},"mt6779",{"$nulls":4},"0x000000FF",0,{"$nulls":12},"mt6779",{"$nulls":19},"0x000000FF",0]