{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["mt6785"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"mt6785","index":0,"n_rows":7,"n_cols":60,"rows_kept":7,"merged":[[0,0,2,0],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,2,4],[0,5,2,5],[0,6,2,6],[0,7,2,7],[0,8,2,8],[0,9,1,59]],"flags":["formulas_cached_only"]}
["Vendor","Part Number","Type","Mode","Density (Mb)","Board ID","NAND/eMMC ID","FW ID","Nand Page Size (B)","MT6768"]
[]
[{"$nulls":9},"CONA_VAL","CHN0_CONA_VAL","CHN1_CONA_VAL","CONF_VAL","CONH_VAL","FREQUENCY","TRAS","TRP","TRPAB","TRC","TRFC","TRFCPB","TXP","TRTP","TRCD","TWR","TWTR","TRRD","TFAW","TRTW_ODT_OFF","TRTW_ODT_ON","REFCNT","REFCNT_FR_CLK","TXREFCNT","TZQCS","TRTPD","TWTPD","TMRR2W_ODT_OFF","TMRR2W_ODT_ON","CHIP_ID","TRAS_05T","TRP_05T","TRPAB_05T","TRC_05T","TRFC_05T ","TRFCPB_05T","TXP_05T","TRTP_05T","TRCD_05T","TWR_05T","TWTR_05T","TRRD_05T","TFAW_05T","TRTW_ODT_OFF_05T","TRTW_ODT_ON_05T","TRTPD_05T ","TWTPD_05T ","TMRR2W_ODT_OFF_05T ","TMRR2W_ODT_ON_05T ","MODE_REG5","PIN_MUX_TYPE"]
["Hynix","H9HQ16AECMMDAR","MCP(UFS+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6785_EVB","0x4839485131364145434d4d444152",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",4266,{"$nulls":23},"mt6785",{"$nulls":19},"0x00000006",0]
["Samsung","KM8V7001JA_B813","MCP(UFS+LPDR4X)","R0_BYTE+R1_BYTE","32768+32768","MT6785_EVB","0x4b4d3856373030314a412d42383133",null,null,"0x03530154","0x0488005D","0x0488005D","0x00421000","0x88880033",3733,{"$nulls":23},"mt6785",{"$nulls":19},"0x00000001",0]
["Hynix","H9HP16AECMMDAR","MCP(eMMC+LPDR4X)","R0_NORMAL+R1_BYTE","16384+32768","MT6785_EVB","0x90014A684445615033",null,null,"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",3733,{"$nulls":23},"mt6785",{"$nulls":19},"0x00000006",0]
["Hynix","H9HQ16AECMMDAR_DIS","Discrete LPDR4X","R0_NORMAL+R1_BYTE","16384+32768","MT6785_EVB",{"$nulls":3},"0x32533154","0x04843059","0x04843059","0x00421000","0x84840023",4266,{"$nulls":23},"mt6785",{"$nulls":19},"0x00000006",0]